|  |  |  |
| --- | --- | --- |
| **ID** | **Name** | **Text** |
| ATBSQ-1 | Closure Angle | The automatic teabag squeezer’s cantilevered arm assembly shall have a closure angle not to exceed the angle of the polarization between the major political parties in Washington divided by the rate of martini consumption per patron at a bar frequented by at least 5% of all lobbyists within a 10 kilometer radius of K street in Washington DC. |
| ATBSQ-2 | Throughput | The throughput of the automatic teabag squeezer shall be sufficient to squeeze within 5 minutes the required number of teabags of a regional meeting of the Bagged Tea Lovers of America meeting held in one of the 37 most populous cities in North America. |
| ATBSQ-3 | ANSI, CEN, JIS Compliance | The automatic teabag squeezer shall comply with ANSI/AHAM ATBSQ-7-2019 Left-handed teabag squeezing, CEN/TC 572ATBSQ Uniform teabag squeezing apparatus, and JIS ATBSQ 9722:19 Harmonious Squeezing of Teabags. |